AalrmModule

# 简介
AalrmModule 是一个报警模块，可以通过扫描数据库中的数据，根据设置的规则进行故障报警的独立程序

# 安装启动
前置条件：需要mysql数据库，linux c环境(centos等)
1.拷贝本项目到服务器,在AlarmModule目录下执行
```
make
```
2.启动服务
```
cd bin
make reboot
```
3.停止服务
```
cd bin
make stop
```
4.查看日志
```
tail -f -n 1000 /tmp/log/xinyun_mqtt_alarm.svr.log
```

# 分析
    考虑到物联网项目中，设备数量和节点数量的不断增多，

    使用之前扫描数据库历史表和逐条解析接收报文方式，会导致性能问题和其他误报警等问题，

    因此采用此方式定时扫描数据库status表，根据设定的阈值规则进行告警判断。

### 项目启动了2个线程
  
  int CoreAlarmGateway() //扫描网关设备数据

  int CoreAlarmNode() //扫描节点设备数据

### 不管是网关还是节点处理的报警逻辑是一样的,报警的类型分以下2大类
  
   1.继电器数据判断(错误码中包括了设备上传的各种报警)
   ```
   //继电器状态:
    #define SW_ON                           0     //0x0000：继电器合闸
    #define SW_MANUAL_CONTROL               32    //0x0020：继电器远程拉闸
    #define SW_TIMER_CONTROL                16    //0x0010: 继电器自动时间段拉闸
    #define SW_TEMPERATURE_HUMIDITY_ALARM   513   //0x0201:继电器温湿度报警拉闸 需报警
    #define SW_FIRE_ALARM                   514   //0x0202:继电器烟感报警拉闸 需报警
    #define SW_TILT_ALARM                   515   //0x0203:继电器倾斜报警拉闸 需报警
    #define SW_LOCK_ALARM                   516   //0x0204:继电器锁具报警拉闸 需报警
    #define SW_LINE_TEMPERATURE_ALARM       517   //0x0205:继电器线温报警拉闸 需报警
    #define SW_OVERVOLTAGE                  1     //0x0001：过压拉闸 需报警
    #define SW_UNDERVOLTAGE                 2     //0x0002：欠压拉闸 需报警
    #define SW_OVERLOAD_ALARM               4     //0x0004: 过载拉闸 需报警
    #define SW_ELECTRIC_EXCESS              8     //0x0008：用电超额拉闸
    #define SW_OVER_SWITCH_OUT_COUNT        64    //0x0040：超自动合闸次数
    #define SW_FAST_CURRENT                 128   //0x0080：快速电流拉闸
   ```
    这部分数据通过RelayAlarm函数处理

   2.结合时间段，拉合闸状态、电流阈值的告警
    + 自动模式合闸时间段继电器拉闸 告警
    + 自动模式拉闸时间继电器合闸    告警
    + 继电器拉闸状态有电流              告警
    + 继电器合闸状态无电流         告警
    + 继电器合闸状态电流偏离正常阈值  告警(需事先采集正常电流最大最小值)

### 报警其他情况排除
   1. 告警dev_fault表计数字段fault_count=3 连续报警3次才会真正报警
   2. dev_status表中新增alarm_enable=0 不报警
   3. 设备在拉合闸相关指令下发的2分钟内，则不进行报警判断
   4. 设备在拉合闸时间点的4个时间点附近2分钟内，则不进行报警判断
   5. 判断过的数据不进行重复读取判断 通过dev_status表标记位electric_update_flag=2
   
### 数据库sql
```
-- 报警清理
UPDATE dev_fault SET fault_state=3

-- 设置设备能报警 SELECT * FROM dev_status WHERE alarm_enable=1
UPDATE dev_status SET alarm_enable=1 where gateway_mac='39FFD7054658383726860743'

----------------------------------------------------------------------------------------------------------------------------------------------------
-- 网关报警数据查询
SELECT t1.device_mac,t1.gateway_mac,t2.device_name,t2.control_mode,t1.update_time,
                t1.current_on_off,t1.current_electric,t1.original_relay,t2.swith_time1,t2.swith_time2,t2.swith_time3,t2.swith_time4,
                t2.electric_wave_set,t2.electric_wave_min,t2.electric_wave_max,t1.command_update_time 
FROM dev_status AS t1 
INNER JOIN dev_info_gateway AS t2 
ON t1.device_mac = t2.device_mac 
WHERE TIMESTAMPDIFF(MINUTE, t1.update_time, NOW()) < 10 
AND t1.current_online=1 
AND t1.original_relay IS NOT NULL 
AND t1.current_electric IS NOT NULL 
AND t1.electric_update_flag=1
AND t1.alarm_enable=1

-- 故障表查询
select device_mac,device_mac_node,fault_state,fault_count,fault_time,relay_code from dev_fault 
where device_mac = '39FFD7054658383726860743' 
and device_mac_node = '0F0000000001'
and relay_code = 1105


-----------------------------------------------------------------------------------------------------------------------------------------------------
-- 节点报警数据查询
SELECT t1.device_mac,t1.gateway_mac,t3.device_name,t2.device_name,t2.control_mode,t1.update_time,t1.current_on_off,t1.current_electric,
       t1.original_relay,t2.swith_time1,t2.swith_time2,t2.swith_time3,t2.swith_time4,t2.electric_wave_set,t2.electric_wave_min,t2.electric_wave_max,t1.command_update_time 
FROM dev_status AS t1 
INNER JOIN dev_info_node AS t2 
ON t1.device_mac = t2.device_mac 
AND t1.gateway_mac=t2.gateway_mac 
INNER JOIN dev_info_gateway AS t3
ON t2.gateway_mac = t3.device_mac 
WHERE TIMESTAMPDIFF(MINUTE, t1.update_time, NOW()) < 10 
AND t1.current_online=1 
AND t1.original_relay IS NOT NULL 
AND t1.current_electric IS NOT NULL 
AND t1.electric_update_flag=1
AND t1.alarm_enable=1

-- 故障表查询
select device_mac,device_mac_node,fault_state,fault_count,fault_time,relay_code from dev_fault 
where device_mac = '39FFD7054658383726860743' 
and device_mac_node = '202105070106' 
and relay_code = 1105
```
